;; NETRTS5.INF (NT 5.0 & Win98 combined inf for NDIS5 driver)
;;
;; Realtek RTL8139 Family PCI/Cardbus Fast Ethernet Network Interface Cards.
;;
;; Copyright 1996-2001, Realtek Semiconductor Corporation
;;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                                 ;;
CatalogFile    = netrts5.cat                               ;; for WHQL certified
CatalogFile.NT = netrtsn.cat
DriverVer      = 08/23/2001,5.397.0823.2001

[Manufacturer]
%Realtek%   = Realtek

[ControlFlags]
ExcludeFromSelect     = PCI\VEN_10EC&DEV_8139
ExcludeFromSelect     = PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC                        

[Realtek]
%RTL8139.DeviceDesc%  = RTL8139.ndi, PCI\VEN_10EC&DEV_8139
%RTL8139_A.DeviceDesc%  = RTL8139_A.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC



;;****************************************************************************
;; Windows 9x
;;****************************************************************************
[rtl8139.ndi]
DriverVer       = 08/23/2001,397
AddReg          = rtl8139.id.reg, RTL8139.common.reg, RTL8139.win.reg, RTL8139.oncbs.reg
CopyFiles       = RTL8139.CopyFiles98
;DeviceID        = "PCI\VEN_10EC&DEV_8139"
;LogConfig       = DefaultConfig

[rtl8139_A.ndi]
DriverVer       = 08/23/2001,397
AddReg          = rtl8139.id.reg, RTL8139.common.reg, RTL8139.win.reg, RTL8139.oncbs.reg
CopyFiles       = RTL8139.CopyFiles98
;DeviceID        = "PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC"
;LogConfig       = DefaultConfig


;;****************************************************************************
;; NT 5.0
;;****************************************************************************
[RTL8139.ndi.NT]
AddReg          = RTL8139.common.reg, RTL8139.reg, RTL8139.oncbs.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8139.CopyFiles

[RTL8139.ndi.NT.Services]
AddService = rtl8139, 2, rtsnt.Service, RTL8139.EventLog

[RTL8139_A.ndi.NT]
AddReg          = RTL8139.common.reg, RTL8139.reg, RTL8139.oncbs.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8139.CopyFiles

[RTL8139_A.ndi.NT.Services]
AddService = rtl8139, 2, rtsnt.Service, RTL8139.EventLog

[RTL8139.CopyFiles]
RTL8139.sys,,,2

[RTL8139.CopyFiles98]
RTL8139.sys,,,2

;;----------------------------------------------------------------------------
;; RTL8139 Parameters
;;----------------------------------------------------------------------------
;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8139.id.reg]
HKR, Ndi,       DeviceID,       0,      "PCI\VEN_10EC&DEV_8139"

HKR, Ndi\Install,                       ,       0,      rtsnt.install
HKR, NDI\Params\DuplexMode,             flag,   1,      30, 00, 00, 00
HKR, Ndi\Params\EarlyTxThreshold,       flag,   1,      20, 00, 00, 00
HKR, NDI\Params\NetworkAddress,         flag,   1,      30, 00, 00, 00
HKR, NDI\Params\WakeUpFrame,            flag,   1,      30, 00, 00, 00

[RTL8139.win.reg]
;; key,subkey,valuname,type,value
HKR, ,  DriverDesc,     0,      "Realtek RTL8139/810X Family PCI Fast Ethernet NIC"
HKR, ,  DevLoader,      0,      *ndis
HKR, ,  DeviceVxDs,     0,      rtl8139.sys
HKR, ,  EnumPropPages,  0,      netdi.dll,      EnumPropPages

;;params
HKR, ,  MediaType,      0,      1
HKR, ,  AdapterType,    0,      5
HKR, ,  BusType,        0,      5

;; NDIS Info
HKR, NDIS,              MajorNdisVersion,       1,      03
HKR, NDIS,              MinorNdisVersion,       1,      0a
HKR, NDIS,              LogDriverName,          0,      "RTL8139"

;; Interfaces
HKR, Ndi\Interfaces,    DefLower,               ,       "ethernet"
HKR, Ndi\Interfaces,    LowerRange,             ,       "ethernet"
HKR, Ndi\Interfaces,    DefUpper,               ,       "ndis3"
HKR, Ndi\Interfaces,    UpperRange,             ,       "ndis3"

;; Install sections
HKR, Ndi\Install,       ndis3,                  0,      "rtl139.ndis5"

;;****************************************************************************
;; RTL8139 common parameters
;;****************************************************************************
[RTL8139.oncbs.reg]
HKR,,ChipOnCardbus,,"0"

[RTL8139.common.reg]
HKR, Ndi\params\DuplexMode,      ParamDesc, 0, %DuplexMode%
HKR, Ndi\params\DuplexMode,      type,      0, "enum"
HKR, Ndi\params\DuplexMode,      default,   0, "1"
HKR, Ndi\params\DuplexMode\enum, 1,         0, %dmAutoMode%
HKR, Ndi\params\DuplexMode\enum, 2,         0, %dm10HalfMode%
HKR, Ndi\params\DuplexMode\enum, 3,         0, %dm10FullMode%
HKR, Ndi\params\DuplexMode\enum, 4,         0, %dm100HalfMode%
HKR, Ndi\params\DuplexMode\enum, 5,         0, %dm100FullMode%

HKR,Ndi\Params\EarlyTxThreshold, ParamDesc, 0, %EarlyTxThreshold%
HKR,Ndi\Params\EarlyTxThreshold, Type,      0, "int"
HKR,Ndi\Params\EarlyTxThreshold, Default,   0, "15"
HKR,Ndi\Params\EarlyTxThreshold, Min,       0, "0"
HKR,Ndi\Params\EarlyTxThreshold, Max,       0, "63"
HKR,Ndi\Params\EarlyTxThreshold, Step,      0, "1"
HKR,Ndi\Params\EarlyTxThreshold, Base,      0, "10"

HKR,Ndi\params\NetworkAddress,   ParamDesc, 0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,   type,      0, "edit"
HKR,Ndi\params\NetworkAddress,   default,   0, "000000000000"
HKR,Ndi\params\NetworkAddress,   LimitText, 0, "12"
HKR,Ndi\params\NetworkAddress,   UpperCase, 0, "1"
HKR,Ndi\params\NetworkAddress,   Optional,  0, "1"

;HKR,NDI\Params\TxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\TxMaxDMABurst,ParamDesc,0,"Transmit DMA burst size"
;HKR,Ndi\params\TxMaxDMABurst,type,0,enum
;HKR,Ndi\params\TxMaxDMABurst,default,0,6
;HKR,Ndi\params\TxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,7,0,"7:2048 bytes"

;HKR,NDI\Params\RxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\RxMaxDMABurst,ParamDesc,0,"Receive DMA burst size"
;HKR,Ndi\params\RxMaxDMABurst,type,0,enum
;HKR,Ndi\params\RxMaxDMABurst,default,0,6
;HKR,Ndi\params\RxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,7,0,"7:unlimitted"

;HKR,NDI\Params\EarlyRxThreshold,flag,1,30,00,00,00
;HKR,Ndi\params\EarlyRxThreshold,ParamDesc,0,"Receive FIFO threshold"
;HKR,Ndi\params\EarlyRxThreshold,type,0,enum
;HKR,Ndi\params\EarlyRxThreshold,default,0,2
;HKR,Ndi\params\EarlyRxThreshold\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,7,0,"7:No threshold"

;HKR,NDI\Params\TxInterFrameGap,flag,1,30,00,00,00
;HKR,Ndi\params\TxInterFrameGap,ParamDesc,0,"Tx IFG(10M/100M)"
;HKR,Ndi\params\TxInterFrameGap,type,0,enum
;HKR,Ndi\params\TxInterFrameGap,default,0,3
;HKR,Ndi\params\TxInterFrameGap\enum,0,0,"8.4us/840ns"
;HKR,Ndi\params\TxInterFrameGap\enum,1,0,"8.8us/880ns"
;HKR,Ndi\params\TxInterFrameGap\enum,2,0,"9.2us/920ns"
;HKR,Ndi\params\TxInterFrameGap\enum,3,0,"9.6us/960ns"

;HKR, Ndi\params\WakeOnLan,         ParamDesc,  0, "Smart Power Saving"
;HKR, Ndi\params\WakeOnLan,         default,    0, "0"  
;HKR, Ndi\params\WakeOnLan,         type,       0, "enum"
;HKR, Ndi\params\WakeOnLan\enum,    "0",        0, "Disable"
;HKR, Ndi\params\WakeOnLan\enum,    "1",        0, "Enable (No WakeUp)"

HKR,Ndi\params\RxBufLen,	   ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,	   type,       0, "enum"
HKR,Ndi\params\RxBufLen,	   default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,	   "0",	       0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "1",	       0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "2",	       0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "3",	       0, "64K bytes"

HKR, Ndi\params\LinkUp,            ParamDesc,  0, "WakeUp on Link Change"
HKR, Ndi\params\LinkUp,            default,    0, "0"
HKR, Ndi\params\LinkUp,            type,       0, "enum"
HKR, Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR, Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR, Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp on ARP/PING"
HKR, Ndi\params\WakeUpFrame,       default,    0, "0"
HKR, Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR, Ndi\params\WakeUpFrame\enum,  "0",        0, "Enable"
HKR, Ndi\params\WakeUpFrame\enum,  "1",        0, "Disable"

HKR, Ndi\params\PME,               ParamDesc,  0, "WakeUp using APM Mode"
HKR, Ndi\params\PME,               default,    0, "1"
HKR, Ndi\params\PME,               type,       0, "enum"
HKR, Ndi\params\PME\enum,          "0",        0, "Enable"
HKR, Ndi\params\PME\enum,          "1",        0, "Disable"

HKR, Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR, Ndi\params\EnableLDPS,        default,    0, "0"
HKR, Ndi\params\EnableLDPS,        type,       0, "enum"
HKR, Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"
HKR, Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"


;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8139.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8139"

[rtsnt.Service]
DisplayName     = %RTL8139.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\RTL8139.SYS
LoadOrderGroup  = NDIS

[RTL8139.EventLog]
Addreg = RTL8139.AddEventLog.reg

[RTL8139.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
RTL8139.CopyFiles           = 12
RTL8139.CopyFiles98         = 11
DefaultDestDir              = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
rtl8139.sys  = 1
;netrts5.inf  = 1
;netrts5.cat  = 1
;netrtsn.cat  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
;Msft                      = "Microsoft"
Realtek                   = "Realtek"

;;Source disk name
DISKNAME = " Realtek RTL8139/810X Family Fast Ethernet NIC Driver Disk "

NetworkAddress            = "Network Address"
EarlyTxThreshold          = "Early Tx Threshold"
DuplexMode                = "Link Speed/Duplex Mode"
dmAutoMode                = "Auto Mode"
dm10HalfMode              = "10 Half Mode"
dm10FullMode              = "10 Full Mode"
dm100HalfMode             = "100 Half Mode"
dm100FullMode             = "100 Full Mode"

RTL8139.DeviceDesc        = "Realtek RTL8139/810X Family PCI Fast Ethernet NIC"
RTL8139.Service.DispName  = "Realtek RTL8139/810X Family PCI Fast Ethernet NIC NT Driver"
RTL8139_A.DeviceDesc      = "Realtek RTL8139/810X Family PCI Fast Ethernet NIC"

;
