# Regulatory Compliance Statements

## Safety Compliance

- UL 60950-1:2001 First Edition
- CAN/CSA-C22.2 No 60950-1-03 First Edition
- EN 60950-1:2001 First Edition (European Union)
- IEC 60950-1:2001 First Edition (International)

## EMC Compliance

- FCC Part 15 – Radiated & Conducted Emissions (USA)
- ICES-003 – Radiated & Conducted Emissions (Canada)
- CISPR 22 – Radiated & Conducted Emissions (International)
- EN55022 – 1998 – Radiated & Conducted Emissions (European Union)
- EN55024 – 1998 – (Immunity) (European Union)
- CE – EMC Directive (89/336/EEC) (European Union)
- VCCI – Radiated & Conducted Emissions (Japan)
- CNS13438 – Radiated & Conducted Emissions (Taiwan)
- AS/NZS3548 – Radiated & Conducted Emissions (Australia/New Zealand)
- MIC notice 1997-41, EMI and MIC notice 1997-42 – EMS (Korea)

## Regulatory Compliance Markings

When required these products are provided with the following Product Certification Markings:

- UL Recognition Mark for USA and Canada
- CE Mark
- FCC markings
- VCCI marking
- Australian C-Tick Mark
- Korea MIC mark
- Taiwan BSMI mark

## Class B Products

### FCC Class B User Information

This equipment has been tested and found to comply with the limits for a Class B digital device pursuant to Part 15 of the FCC rules. These limits are designed to provide reasonable protection against harmful interference in a residential installation. This equipment generates, uses and can radiate radio frequency energy and, if not installed and used in accordance with the instructions, may cause harmful interference to radio communications. However, there is no guarantee that interference will not occur in a particular installation.

If this equipment does cause harmful interference to radio or television reception, which can be determined by turning the equipment off and on, the user is encouraged to try to correct the interference by one or more of the following measures:

- Reorient or relocate the receiving antenna.
- Increase the separation between the equipment and receiver.
- Connect the equipment into an outlet on a circuit different from that to which the receiver is connected.
- Consult the dealer or an experienced radio/TV technician for help.

| CAUTION: If the device is changed or modified without permission from Intel, the user may void his or her authority to operate the equipment.

| NOTE: This device complies with Part 15 of the FCC Rules. Operation is subject to the following two conditions: (1) this device may not cause harmful interference, and (2) this device must accept any interference received, including interference that may cause undesired operation.

### Copper Products

- Intel® PRO/1000 XT Server Adapter
- Intel® PRO/1000 T Server Adapter
- Intel® PRO/1000 MT Server Adapter
- Intel® PRO/1000 MT Dual Port Server Adapter
- Intel® PRO/1000 P Dual Port Server Adapter
- Intel® PRO/1000 GT Dual Port Server Adapter
- Intel® PRO/1000 PT Server Adapter
- Intel® PRO/1000 PT Dual Port Server Adapter
- Intel® PRO/1000 GT Quad Port Server Adapter
- Intel® PRO/1000 PT Quad Port Server Adapter
- Intel® PRO/1000 PT Quad Port LP Server Adapter

## Electromagnetic Compatibility Notices

### FCC Declaration of Conformity Statement

The PRO/1000 XT Server Adapter, PRO/1000 MT Server Adapter, PRO/1000 MT Dual Port Server Adapter, PRO/1000 T Server Adapter, and PRO/1000 P Dual Port Server Adapter have been tested to Comply with FCC Standards for Home or Office Use.

Intel Corporation, Mailstop JF3-446
5200 N.E. Elam Young Parkway
Hillsboro, OR 97124-6497
Phone 1-800-628-8686

### Fiber Products

(Verified for FCC Class B)

- Intel® PRO/1000 F Server Adapter
- Intel® PRO/1000 XF Server Adapter
- Intel® PRO/1000 MF Server Adapter (LX)
- Intel® PRO/1000 MF Server Adapter
- Intel® PRO/1000 MF Dual Port Server Adapter
- Intel® PRO/1000 PF Server Adapter
- Intel® PRO/1000 PF Dual Port Server Adapter
- Intel® PRO/1000 PF Quad Port Server Adapter

## Canadian Compliance (Industry Canada)

CANADA ICES-003 CLASS B / CANADA NMB-003 CLASSE B

## VCCI Class B Statement (Japan)

## MIC Notice Class B (Republic of Korea Only)

## BSMI Class A Notice (Taiwan)

## China RoHS Declaration

## Manufacturer Declaration
European Community

## Manufacturer Declaration

Intel Corporation declares that the equipment described in this document is in conformance with the requirements of the European Council Directive listed below:

73/23/EEC Low Voltage Directive with Amendment 93/68/EEC
89/336/EEC EMC Directive with Amendments 92/31 EEC and 93/68/EEC

This product follows the provisions of the European Directive 1999/5/EC.

Dette produkt er i overensstemmelse med det europæiske direktiv 1999/5/EC.

Dit product is in navolging van de bepalingen van Europees Directief 1999/5/EC.

Tämä tuote noudattaa EU-direktiivin 1999/5/EC määräyksiä.

Ce produit est conforme aux exigences de la Directive Européenne 1999/5/EC.

Dieses Produkt entspricht den Bestimmungen der Europäischen Richtlinie 1999/5/EC.

Þessi vara stenst reglugerð Evrópska Efnahags Bandalagsins númer 1999/5/EC.

Questo prodotto è conforme alla Direttiva Europea 1999/5/EC.

Dette produktet er i henhold til bestemmelsene i det europeiske direktivet 1999/5/EC.

Este produto cumpre com as normas da Diretiva Européia 1999/5/EC.

Este producto cumple con las normas del Directivo Europeo 1999/5/EC.

Denna produkt har tillverkats i enlighet med EG-direktiv 1999/5/EC.

This declaration is based upon compliance of the product to the following standards:

EN 55022 (CISPR 22 Class B) RF Emissions Control.
EN 55024 Immunity to Electromagnetic Disturbance.
EN 60950-1 First Edition Information Technology Equipment- Safety-Part 1: General Requirements.

Intel Corporation, Mailstop JF3-446
5200 N.E. Elam Young Parkway
Hillsboro, OR 97124-6497
Phone 1-800-628-8686

# Class 1 Laser Product

The PRO/1000 F, PRO/1000 XF, and PRO/1000MF Server Adapters contain laser devices for communication use. These devices are compliant with the requirements for Class 1 Laser Products and are safe in the intended use. In normal operation the output of these laser devices does not exceed the exposure limit of the eye and cannot cause harm.

For continued safe operation in case of an abnormal circumstance, always have the provided laser connector cover in place or a compatible fiber optics cable properly connected when power is available to the product.

The Laser device must be factory serviced ONLY by the responsible manufacturer! NO adjustments, service or maintenance is to be performed otherwise.

| CAUTION: Use of controls or adjustments or performance of procedures other than those specified herein may result in hazardous radiation exposure.

## These Class 1 Laser devices:

Comply with FDA/CDRH per CFR21, subchapter J.

Comply with IEC 60825-1(1993)/A2:2001 and EN60825-1:1994+A11+A2

`Last modified on 12/12/06 4:20p Revision 14`