# SNMP Agent Extension for NetWare*

Overview

Prerequisites

Installation Instructions

Available Commands

## Overview

The LANAgent module extends the SNMP agent for NetWare* to provide information on Intel adapters.

The following information describes how to enable the NetWare SNMP module to support the INTEL® LAN ADAPTERS MIB.

## Prerequisites

For optimal performance by the SNMP agent, install the appropriate NetWare drivers:

- For 100 adapters: ce100.lan
- For Gigabit PCI-X adapters: e1000.lan
- For Gigabit PCI-Express adapters: e1000e.lan

The SNMP agent package is compliant with the following driver versions:

- CE100b.lan: ver 4.11 and above
- E1000.lan: ver 3.03 and above
- E1000E.lan: ver 3.03 and above
- iANS.lan : ver 4.14 and above

## Installation Instructions

1. At the server prompt enter:

   > Load <path\>LANAgent

2. Configure the SNMP community name according to the Novell* documentation. For example, to enable GET and SET for any community name enter:

   > Load SNMP ControlCommunity=

   For more information, go to http://support.novell.com.

3. Register to receive Traps by adding the IP address of the management station to the list in the SYS:\ETC\TRAPTARG.CFG file.

## Available Commands

Command | Default | Description
-h help | n/a | View the help description.
cache_time=<nn> | 50 (5 seconds) | Define a time period in which the data structure is considered valid. Two consecutive queries within that time will not cause update of the data. <nn> is an integer value set to 1/10 second.
trap_time=<nn> | 10 (1 second) | Define the time period between two consecutive trap checks. The units are the same as for cache_time.
status | n/a | View the current values for cache_time and trap_time.

`Last modified on 3/08/07 10:42a Revision 7`