REGEDIT4

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL]

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices]
"Supported"=dword:00000003
"SMBus"=dword:00000001

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device1]
"Name"="SMSC LPC47M15X Temperature Monitor Device"
"BaseAddress"=dword:0000002d
"Fans Muxed"=dword:00000000
"FanMuxAddress"=dword:00000000
"Pixx4 Muxed"=dword:00000000
"Pixx4ClrGPIO"=dword:00000000
"Pixx4SetGPIO"=dword:00000000
"ConfigurationRegAddr"=dword:00000040
"StatusRegAddr"=dword:00000041
"ClrRegAddr"=dword:00000046
"VIDRegAddr"=dword:00000047
"BusType"=dword:00000000
"AsicType"=dword:00000014
"Support"="F"
"HecetaVersion"=dword:00000000
"CTRRegister"=dword:00000000
"DriverType"=dword:00000001

"DriverType"=dword:00000001

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device1\Fans]
"Supported"=dword:00000002

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device1\Fans\Fan1]
"Address"=dword:00000029
"MaxThreshAddr"=dword:00000000
"MinThreshAddr"=dword:0000003c
"Nominal"=dword:00000b90
"StatusBit"=dword:00000000
"MaxThreshold"=dword:00000000
"MinThreshold"=dword:000005dc
"Granularity"=dword:00000000
"Description"=dword:00000006
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000001
"Muxed"=dword:00000000
"GPIO Value"=dword:000000ff
"Tach Input"=dword:00000002
"AutoDetect"=dword:00000000
"Enabled"=dword:00000001
"CTRBit"=dword:00000000
"CTRValue"=dword:00000000
"CTRValue"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device1\Fans\Fan2]
"Address"=dword:00000028
"MaxThreshAddr"=dword:00000000
"MinThreshAddr"=dword:0000003b
"Nominal"=dword:00000bb8
"StatusBit"=dword:00000000
"MaxThreshold"=dword:00000000
"MinThreshold"=dword:000005dc
"Granularity"=dword:00000000
"Description"=dword:00000006
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000001
"Muxed"=dword:00000000
"GPIO Value"=dword:000000ff
"Tach Input"=dword:00000002
"AutoDetect"=dword:00000001
"Enabled"=dword:00000000
"CTRBit"=dword:00000000
"CTRValue"=dword:00000000
"CTRValue"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device1\Voltages]
"Supported"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device1\Temperatures]
"Supported"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device1\Intrusions]
"Supported"=dword:00000000


[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2]
"Name"="SMSC LPC47M15X SMBus Temperature and Voltage Monitor Device"
"BaseAddress"=dword:0000002d
"Fans Muxed"=dword:00000000
"FanMuxAddress"=dword:00000000
"Pixx4 Muxed"=dword:00000000
"Pixx4ClrGPIO"=dword:00000000
"Pixx4SetGPIO"=dword:00000000
"ConfigurationRegAddr"=dword:00000040
"StatusRegAddr"=dword:00000041
"ClrRegAddr"=dword:00000046
"VIDRegAddr"=dword:00000047
"BusType"=dword:00000000
"AsicType"=dword:00000011
"Support"="TV"
"HecetaVersion"=dword:00000000
"CTRRegister"=dword:00000000
"DriverType"=dword:00000000

"DriverType"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Fans]
"Supported"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Voltages]
"Supported"=dword:00000006

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Voltages\Voltage1]
"Address"=dword:00000023
"MaxThreshAddr"=dword:00000031
"MinThreshAddr"=dword:00000032
"Nominal"=dword:00001388
"StatusBit"=dword:00000000
"MaxThreshold"=dword:00004e20
"MinThreshold"=dword:00000000
"Granularity"=dword:00009600
"Description"=dword:00000003
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000001
"AutoDetect"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Voltages\Voltage2]
"Address"=dword:00000024
"MaxThreshAddr"=dword:00000033
"MinThreshAddr"=dword:00000034
"Nominal"=dword:00002ee0
"StatusBit"=dword:00000000
"MaxThreshold"=dword:0000c350
"MinThreshold"=dword:00000000
"Granularity"=dword:00003e80
"Description"=dword:00000001
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000001
"AutoDetect"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Voltages\Voltage3]
"Address"=dword:00000022
"MaxThreshAddr"=dword:0000002f
"MinThreshAddr"=dword:00000030
"Nominal"=dword:00000ce3
"StatusBit"=dword:00000000
"MaxThreshold"=dword:00007350
"MinThreshold"=dword:00000000
"Granularity"=dword:0000e344
"Description"=dword:00000005
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000001
"AutoDetect"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Voltages\Voltage4]
"Address"=dword:00000051
"MaxThreshAddr"=dword:00000056
"MinThreshAddr"=dword:00000057
"Nominal"=dword:00000707
"StatusBit"=dword:00000000
"MaxThreshold"=dword:00004e20
"MinThreshold"=dword:00000000
"Granularity"=dword:0001a0ae
"Description"=dword:0000000a
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000001
"AutoDetect"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Voltages\Voltage5]
"Address"=dword:00000050
"MaxThreshAddr"=dword:00000054
"MinThreshAddr"=dword:00000055
"Nominal"=dword:000005dc
"StatusBit"=dword:00000000
"MaxThreshold"=dword:00002710
"MinThreshold"=dword:00000000
"Granularity"=dword:0001f400
"Description"=dword:0000000b
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000001
"AutoDetect"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Voltages\Voltage6]
"Address"=dword:00000021
"MaxThreshAddr"=dword:0000002d
"MinThreshAddr"=dword:0000002e
"Nominal"=dword:0000056e
"StatusBit"=dword:00000000
"MaxThreshold"=dword:00002710
"MinThreshold"=dword:00000000
"Granularity"=dword:00014a5a
"Description"=dword:0000000c
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000001
"AutoDetect"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Temperatures]
"Supported"=dword:00000001

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Temperatures\Temperature1]
"Address"=dword:00000052
"MaxThreshAddr"=dword:00000058
"MinThreshAddr"=dword:00000059
"Nominal"=dword:0000001e
"StatusBit"=dword:00000000
"MaxThreshold"=dword:00000050
"MinThreshold"=dword:00000000
"Granularity"=dword:000003e8
"Description"=dword:00000006
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000001
"UsesBanks"=dword:00000000
"BankAAddr"=dword:0000005d
"BankBAddr"=dword:00000059
"BankABit"=dword:00000001
"BankBBit"=dword:00000001
"BankABitValue"=dword:00000001
"BankBBitValue"=dword:00000001

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device2\Intrusions]
"Supported"=dword:00000000


[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device3]
"Name"="Chipset TCO"
"BaseAddress"=dword:00000060
"Fans Muxed"=dword:00000000
"FanMuxAddress"=dword:00000000
"Pixx4 Muxed"=dword:00000000
"Pixx4ClrGPIO"=dword:000000ff
"Pixx4SetGPIO"=dword:000000ff
"ConfigurationRegAddr"=dword:00000040
"StatusRegAddr"=dword:00000041
"ClrRegAddr"=dword:00000046
"VIDRegAddr"=dword:00000047
"BusType"=dword:00000002
"AsicType"=dword:00000012
"Support"="C"
"HecetaVersion"=dword:00000000
"CTRRegister"=dword:00000000
"DriverType"=dword:00000000

"DriverType"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device3\Fans]
"Supported"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device3\Voltages]
"Supported"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device3\Temperatures]
"Supported"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device3\Intrusions]
"Supported"=dword:00000001

[HKEY_LOCAL_MACHINE\Software\Intel\LANDesk\SMAL\AsicDevices\Device3\Intrusions\Intrusion1]
"Address"=dword:00000006
"MaxThreshAddr"=dword:00000006
"MinThreshAddr"=dword:00000000
"Nominal"=dword:00000000
"StatusBit"=dword:00000000
"MaxThreshold"=dword:00000000
"MinThreshold"=dword:00000000
"Granularity"=dword:00000000
"Description"=dword:0000000d
"Poll Frequency"=dword:000003e8
"Capability"=dword:00000000
"ClearBit"=dword:00000000

[HKEY_LOCAL_MACHINE\Software\Intel\cimgr\Instrumentation.IOSMAL.2.1\Chassis\Health Contributor|Intrusion Detection|001\state]
"OKState"=dword:00000000


[HKEY_LOCAL_MACHINE\System\CurrentControlSet\Services\smbusp\Parameters]
"TakeInUse"=dword:00000001
"TakeInUseOnStart"=dword:00000001