
Usage:
1. Connect the video phone and PC with a network cable, or you could connect the video and PC to a same Hub or Switch.

2. Set the PC's network property as:
    IP Address ：192.168.0.23
	NetMask    ：255.255.240.0
	GateWay	   ：192.168.0.3
	
3. run "clickhere.bat"

4. Power on the phone and at the same time long press F2 key on the video phone.(it's not the F2 key on the PC). Seconds later, you will see the phone go to update. If it fails, try again. Please press the F2 key as soon as you power on the phone.

FAQ:
Q1. which key is F2 on VP2009?
A: There're 4 buttons on VP2009D at the top of the keyboard. Counted from the left, they are F1, F2, F3, F4. So the top left second key is F2.

Note:
When updating, there will be some Chinese characters in the ftp20CN,reg, but you don't need to do any operation in it.











1.设置网络环境
	用一条网线将VideoPhone跟PC对连，使其网络互通，可直接接在同个Hub或交换机上。
	设置PC的网络属性 
	IP Address ：192.168.0.23
	NetMask    ：255.255.240.0
	GateWay	   ：192.168.0.3

2.执行操作
	(1)运行“点这里.bat”
	(2)在给可视电话上电的同时，长按可视电话上的F2按键。如果不成功，多可尝试几次，记住一定要尽快按下可视电话上的F2键
	(3)可将同个网络中的多台设备同时进行F2升级
	
键盘上，上方左起第二个键是F2。
	
